침엽수림에서의 지상LiDAR를 이용한 산림조사 활용성 평가

고병준1*, 박세익1, 이상현2

(1전북대학교 임학과, 2전북대학교 산림환경과학과)

Evaluation of Utilization for Forest Inventory

Using Terrestrial LiDAR in Coniferous Forest

Byung-Jun Ko1*, Se-Ik Park1, Sang-Hyun Lee2

(1Department of Forestry, Jeonbuk National University,

2Department of Forest Environment Science, Jeonbuk National University)

요약: 본 연구는 침엽수림에서 입목의 수고와 흉고직경 측정에 있어 조사원이 직접 측정하는 기존의 방법과 지상 LiDAR를 이용하여 측정하는 방법의 차이를 비교분석을 통하여 지상 LiDAR의 활용성을 평가하였다. 지상 LiDAR는 운용 방식이 다른 지상 LiDAR 간의 정확도를 비교하기 위하여 고정식과 이동식을 사용하였으며, 비교분석은 대응표본 t-test, 상관관계 분석, Bland-Altman 그래프 분석 방법을 이용하였다. 수고의 경우 기존의 방법으로 측정한 값과 지상 LiDAR로 측정한 값 간의 차이 평균값은 고정식이 0.81m, 이동식이 2.88m로 나타났으며, 흉고직경의 경우 고정식이 0.13cm, 이동식이 2.36cm로 나타났다. 따라서 차이 평균값이 0에 더 근접한 고정식 지상 LiDAR를 이용한 측정 방법이 기존의 측정 방법과 일치성이 높은 것으로 나타났다. 침엽수림에서 지상 LiDAR를 이용한 측정에 미치는 영향은 지상 LiDAR의 운용 방식과 사양으로 나타났다.

Abstract: This study objective is to evaluate of forest inventory using terrestrial LiDAR in coniferous forest by comparing and analyzing the difference between the traditional measurement method by person and the measurement method using terrestrial LiDAR. The terrestrial LiDAR used fixed type and handy type with different operational methods to compare their accuracy at coniferous forest. Comparative analyses was used a paired t-test, correlation analysis, and Bland-Altman plot analysis methods. In the case of tree heights, the average value of the difference between traditional methods and terrestrial LiDAR was shown to be 0.81m for fixed type, 2.88m for handy type. In the case of tree diameters at breast height, the average value of the difference between traditional methods and terrestrial LiDAR was shown to be 0.13cm for fixed type, 2.36cm for handy type. Therefore, it has been shown that the method using fixed type terrestrial LiDAR is highly consistent with traditional measurement methods because the difference average value is closer to zero than the method using handy type terrestrial LiDAR. The impact on the method using terrestrial LiDAR was shown to be operation and specification of terrestrial LiDAR.

Keyword: Terrestrial LiDAR, TLS, Forest inventory, Coniferous forest, Bland-Altman plot