땅밀림 발생지의 상대적 위험도 평가방안에 관한 연구

서준표*, 이창우, 우충식, 유송, 이기환, 강민정

(국립산림과학원 산림보전연구부 산림방재연구과)

A Study on the Evaluation of the Relative Risk of Slow-moving landslide

Junpyo Seo*, Changwoo Lee, Choongshik Woo, Song Eu, KiHwan Lee, Minjeng Kang

(Division of Forest Disaster Management, Department of Forest Conservation,
National Institute of Forest Science)

요약: 국내에서 산지토사재해로 인한 피해는 산사태와 토석류가 대부분이지만 2017년 포항지진 이후에는 땅밀림에 대한 위험성이 대두되어 관련 연구개발이 활발히 수행되고 있다. 땅밀림은 강우나 지하수에 의해 산지비탈면이 포화되고 중력작용에 의하여 느린 속도로 이동하는 현상을 말한다. 국내에 알려진 땅밀림 발생지는 35개소인데 이에 대한 복구 등 관리대책이 필요하다. 그러나 한정된 인력과 예산을 효율적으로 활용하기 위해서는 상대적 위험성 평가를 통해 복구 우선순위를 결정할 필요가 있다. 본 연구에서는 땅밀림 발생지에 대한 상대적 위험도를 정량적으로 평가하기 위하여 사면안정해석법을 적용하였다. 분석에는 건축·지반 등 현장에서 많이 사용되고 있는 Bishop의 간편법(한계평형법)을 사용하였고, 과학적 분석을 위하여 물리탐사(탄성파탐사)와 토질분석(점착력, 내부마찰각 등) 자료가 있는 14개소를 대상으로 안정해석을 수행하였다. 건설공사 비탈면 설계기준의 허용안전율 건기 1.5, 우기 1.2 이상을 기준안전율로 하였다. 그 결과 건기 평균 안전율 1.7, 우기 평균 안전율 0.8로 건기에 7개소(50%), 우기에 12개소(85%)가 불안정한 것으로 분석되었으며, 안전율과 같은 정량적 수치를 도출함으로써 땅밀림에 대한 서열화로 위험도 우선순위 선정이 가능한 것으로 판단된다.

Abstract: Most of the damage caused by mountainous soil disasters in Korea is landslides and debris flow, but related research and development have been actively carried out since the 2017 Pohang earthquake due to the danger to the slow-moving landslide. A slow-moving landslide is a phenomenon in which mountain slopes are saturated by rainfall or groundwater and moved at a slow rate due to gravitational action. There are 35 slow-moving landslide sites known in Korea, and management measures such as rehabilitation are needed. However, in order to efficiently utilize limited manpower and budgets, it is necessary to determine rehabilitation priorities through relative risk assessments. In this study, the slope stability analysis was applied to quantitatively evaluate the relative risk of slow-moving landslide sites. The analysis was conducted using the Bishop's method, which is widely used in the field, and the slope stability analysis was conducted on 14 sites with physical exploration and soil analysis data for scientific analysis. The permitted safety rate of the construction slope design standards was dry season 1.5, rainy season 1.2, or more as a reference safety rate. As a result, the average safety rate of the dry season was 1.7 and the average safety rate of the rainy season was 0.8, which was analyzed to be 7 sites (50%) in the dry season and 12 sites (85%) in the rainy season. And by deriving quantitative figures such as slope safety factor, it is determined that risk is possible to select priority by ranking for the slow-moving landslide.