영상 모니터와 실제작업에 따른 원목 상차작업 생산성 비교 분석

최윤성1*, 정인선1, 조민재1, 문호성1, 오재헌1

(1국립산림과학원 산림기술경영연구소)

Comparative Analysis of Loading Productivity between Operation with Image Monitor and Actual Operation

Yun-Sung Choi1*, In-Seon Jeong1, Min-Jae Cho1, Ho-Seong Mun1, Jae-Heun Oh1

(1Forest Technology and Management Research Center, National Institute of Forest science)

요약: 본 연구는 굴삭기 우드그랩과 궤도형 임내차를 이용하여, 영상 모니터와 실제작업에 따른 원목 상차작업 생산성을 비교·분석하였다. 작업자 A, B(경력 30년 이상, 50대), 작업자 C(경력 5년 이하, 30대), 작업자 D(경력 5년 이하, 20대)로 구분하였으며, 장비위치를 고정하여 동일한 조건으로 잣나무 원목 2.1m를 상차작업하였다. 작업자별 영상 모니터와 실제작업에 따른 상차작업 생산성은 통계적으로 유의한 차이가 있는 것으로 분석되었다(p<0.05). 실제 상차작업의 생산성은 작업자 B(27.5톤/시간), 작업자 D(22.8톤/시간), 작업자 A(16.2톤/시간), 작업자 C(15.2톤/시간)로 나타났다. 영상 모니터작업의 상차작업 생산성은 작업자 D(15.1톤/시간), 작업자 B(12.4톤/시간), 작업자 A(9.8톤/시간), 작업자 C(9.5톤/시간)로 나타났다. 실제 상차작업 생산성은 경력이 높은 작업자 B가 작업자 D보다 높게 나타났으나, 영상 모니터의 상차작업 생산성은 작업자 D가 작업자 B보다 높게 나타났다. 영상 모니터의 상차작업은 연령과 상관관계가 높은 것으로 사료되며, 향후 경력과 연령을 모두 고려한 정밀 분석을 위해 추가 연구가 필요할 것으로 판단된다.

Abstract: This study used excavator-based wood grapple loader and forwarder, and compared and analyzed the productivity of loading operation according to image monitor and actual operation. The operator A and B(30 years of experience or more, 50s), operator C(5 years of experience or less, 30s) and operator D(5 years of experience or less, 20s). The equipment location was fixed, and 2.1 m of pinus koraiensis log was loaded under the same condisions. It was analyzed that there was a statistical significant difference in the loading productivity of image monitor and actual operation(p<0.05). In the autual loading operation, the productivity was operator B(27.5 t/hr), operator D(22.8 t/hr), operator A(16.2 t/hr), and operator(15.2 t/hr). In the image monitor loading operation, the productivity was operator D(15.1 t/hr), operator B(12.4 t/hr), operator A(9.8 t/hr), and operator C(9.5 t/hr). In the autual loading operation, the productivity was operator B(high-experience) was higher than operator D, and the image monitor loading operation, the productivity was operator D was higher than operator B. In the image monitor, loading operation was considered to have a high correlation with age. Therefore, additional study was expected to be needed for a detailed analysis that considers both experience and age in the future.

사사 : 본 연구는 국립산림과학원 일반과제(FO0200-2018-01)의 지원에 의해 이루어진 것임.