용기 종류, 생육상토, 관수량이 거제수나무의 생장에 미치는 효과

박소라*, 안지영, Myo Min Latt, Hernandez O. Jonathan, Ser-Oddamba Byambadorj, 한시호, 박병배

(충남대학교 산림자원학과)

Effects of pot types, soil types, and the volume of irrigation

on growth performance of Betula costata Trautv.

Sora Park*, Ji Young An, Myo Min Latt, Hernandez O. Jonathan, Ser-Oddamba Byambadorj,

Si Ho Han, Byung Bae Park.

(Department of Environment and Forest Resources, Chungnam National University)

요약: 용기종류와 생육상토에 따른 관수조건은 경관 또는 도시숲 조성용 수목의 생산품질에 절대적인 영향을 미친다. 본 연구는 거제수나무(Betula costata Trautv.)를 대상으로 일반용기(플라스틱, 35 L), 에어포트(공기단근용기, 35 L) 2종 × 일반상토, 혼합상토(상토:마사토=7 : 3 비율), 마사토 3종의 6조합처리에 다양한 관수량(36 mL/hour/pot ∼ 4017 mL/hour/pot)을 처리하였다. 수고와 근원경 생장률은 에어포트가 일반용기보다 1.7배, 바이오매스는 1.8배 더 높게 나타났다. 에어포트 처리에서  혼합상토가 마사토보다 수고생장률이 1.8배, 근원경 생장률은 2.6배, 바이오매스는 2.5배 더 높았다. 에어포트와 마사토는 통기성과 배수성을 높이고, 수목생산비용 절감 효과를 기대하면서 수목품질을 유지할 수 있는 방법이지만 이에 따른 관수량은 일반용기와는 다르게 적용되어야 한다. 6조합처리에서 관수량이 500 mL/hour/pot 이상일 때는 생장의 증가가 완만하였지만 300 mL/hour/pot 이하로 매우 적을 경우 생장 감소가 나타났다. 이러한 경향은 특히 에어포트와 마사토 처리에서 뚜렷하였다. 본 연구가 공원녹지와 가로수 등 도시숲 형성에 적합한 중형수목 생산의 재배조건을 제시하여 도시환경을 개선하는데 활용될 수 있기를 기대한다.

Abstract: The types of containers, soil, and conditions of irrigation have an impact on the quality of trees in urban forests. Two types of containers(35 L): plastic and airpots, and three types of soil(bedsoil, mixed soil with the ratio of bedsoil to loamy sand of 7 : 3, and loamy sand)were used to produce Betula costata Trautv. The volume of irrigation was varied from 36 mL/hour/pot to 4017 mL/hour/pot. Airpots displayed a growth rate 1.7 times higher than that of plastic containers in both height and RCD. The biomass was 1.8 times higher. In the case of airpots, the mixed soil had a growth rate 1.8 times and 2.6 times higher for height and RCD. Airpots and loamy sand help to increase ventilation and to maintain the quality of trees while reducing the cost of producing trees. However, irrigation should be applied differently to these arrangements. The growth rate was moderate when the irrigation was over 500 mL/hour/pot, it fell if the irrigation was below 300 mL/hour/pot. This trend was evident in the airport and loamy sand. It is hoped that this study will present ideal conditions for the cultivation of medium-sized trees, suitable for urban forests, and be used to improve urban environments. Keywords: Betula costata, Urban forest, Airpot, Growth media, Growth performance.

사사: 본 연구는 산림청(한국임업진흥원) 산림과학기술 연구개발사업 ‘(FTIS 2020173C10 - 2023 - AD01)’의 지원에 의해 이루어진 것입니다.