산림 미세먼지 측정넷 기반 그린 쉘터 탐색을 위한 보행 네트워크 개발

박완혁1,2*, 박찬열1, 송동하3, 최수민1, 고동욱2

(1국립산림과학원 도시숲연구센터, 2국민대학교 산림자원학과, 3스마클(주))

Development of Walking Networks for Green Shelters based on the Forest PM Monitoring-Net

Wanhyeok Park1,2, Chan-Ryul Park1, Dongha Song3, Sumin Choi1, Dongwook W. Ko2

(1Urban Forests Research Center, National Institute of Forest Science,

2Department of Forest Resources, Kookmin University, 3Smarcle Co. Ltd.)

요약: 국립산림과학원은 2020년까지 20개소 60지점의 미세먼지 측정넷을 구축하였다. 각 측정소는 오염원과의 거리에 따라서 3개 측정점을 포함하고 있다. 3개 측정점을 기반으로 측정소 전체 지역(직경 4km)에서 고농도 및 폭염시기에 대피할 수 있는 ‘숨편한길’과 ‘더위피하는길’을 도출하기 위한 보행 경로를 개발하였다. 조사지역내 그린/그레이 인프라, 생활인구, 토지피복, 지형 등을 분석하였다. 그린쉘터는 학교숲, 도시숲, 공원 등으로 설정하였다. 보행 속도, 보도 인근 생활인구, 주변 통행량, 토지피복도, 미세먼지 실측값을 종합하여 보행 점수에 가중치를 부여했다. 100m 간격의 인구 데이터를 구역 통계를 이용해 건물에 할당하여 생활인구 지도를 작성하고 보도 주변 반경 10m 이내의 생활인구와 통행량을 합산하여 많을수록 낮은 등급을 부여하였다. 토지피복 유형별로 보행자 선호도를 고려하여 점수를 차등 적용하였다. 미세먼지 ‘나쁨’ 날짜에 실측된 데이터를 종합하여 그린쉘터간 미세먼지 노출을 최소로 하는 경로 네트워크를 산출하였다. 향후, 측정넷의 실측 데이터를 기반으로 실시간 예보 등으로 응용이 가능할 것으로 보인다.

Abstract: The National Institute of Forest Science has established a PM(particulate matter) monitoring net at 60 points in 20 stations by 2020. Each Monitoring station contains three monitoring points depending on the distance from the pollutant source. In the area within 2 km radius of each monitoring station, a walking network was developed to derive “easy-breathing-pathway” and a “avoiding-heat-pathway” that can be a refuge during the period of high concentration of PM and heat wave. The green/gray infrastructure, living population, land cover, and topography were analyzed in the study area. School forests, urban forests, and parks were set up as “green shelters”. Walking speed, living population and traffic volume near the walkway, land cover, and the measured data of PM were synthesized to ranks weight value to the walking score. Population data were allocated to buildings to create a living population map. And the living population and traffic volume were summed up within 10 m around the walkway. A low grade was given to high-value segments. The walking network that minimizes the exposure of PM between green shelters was calculated by synthesizing the data measured on the high PM concentration date.

Keywords: PM reduction, Public Awareness, Spatial Modeling, Urban Forests

사사: 본 연구는 국립산림과학원 ‘미세먼지 저감 도시숲 가치의 측정넷 기반 대국민 인식증진 기술 개발’과제(No.FE0100-2019-06-2021)에서 수행한 연구 결과임.