산불 식생피해강도가 토양 투수계수에 미치는 영향

이기문1*, 안수정2,3, 김태현1, 이제만1, 임상준1,4

(1서울대학교 농림생물자원학부, 2강원도 동해안산불방지센터,

3국립산림과학원 산림방재연구과, 4서울대학교 농업생명과학연구원)

Post-fire Impact of Vegetation Burn Severity on Saturated Hydraulic Conductivity of Soil

Qiwen Li1*, Sujung Ahn2,3, Tae Hyun Kim1, Jeman Lee1, Sangjun Im1,4

(1Department of Agriculture, Forestry and Bioresources, Seoul National University,

2East Coastal Forest Fire Center of Gangwon Province,

3Division of Forest Disaster Management, National Institute of Forest Science,

4Research Institute of Agriculture and Life Sciences, Seoul National University)

요약: 이 연구는 산불 식생피해강도가 산불에 의해 생성된 산불 토양의 물리적·수리적 특성에 미치는 영향을 알아보고자 진행하였다. 토양 채취를 위해 현행 산불 식생피해 분류에 의해 미피해, 지표화, 수관열해, 수관화 등 네 가지 지역으로 구분하여 각 지역마다 3점의 표층토양(0-5 cm)을 수집한 후 변수위법으로 토양의 투수계수를 측정하였다. 측정결과, 미피해, 지표화, 수관열해, 수관화 지역의 투수계수는 각각 0.008969, 0.003828, 0.001966, 0.001553 cm/s로 나타나 전반적으로 감소하는 경향을 보였다. 분산분석 결과, 지표화, 수관열해, 수관화 지역과 미피해 지역에서 p<0.05 수준에서 유의한 차이를 보였으나 지표화, 수관열해 및 수관화 지역 사이에서는 유의성 수준을 만족하지 않아 차이가 없는 것으로 판단되었다.

Abstract: This study investigated the direct impacts of forest fires on soil hydraulic properties with vegetation burn severity. Soil samples were collected in four stratified units which were unburned (UB), surface-fuel consumption (SC), foliage necrosis (FN) and crown-fuel consumption (CC). The saturated hydraulic conductivity were measured by fall-head method. The results showed that mean saturated hydraulic conductivities in each area were 0.008969, 0.003828, 0.001966, 0.001553 cm/s, respectively. Non-parametric ANOVA showed that saturated hydraulic conductivity in UB area was significantly different from the other areas (p<0.05), while among SC, FN and CC areas were not. A decrease, nevertheless, in hydraulic conductivity was observed with vegetation burn severity.

사사: 이 논문은 정부(과학기술정보통신부)의 재원으로 한국연구재단의 지원을 받아 수행된 연구임(No. 2019R1A2C1089203).