낙엽송 임분의 개벌작업에 있어서 전목 및 단목 수확시스템의

작업생산성 및 비용분석

정응진1, 조현민1, 이영석1, 한상균1*

(1강원대학교 산림환경과학대학 산림과학부)

Comparative Analysis of Operation Productivity and Costs between Whole-tree and Cut-to-Length Harvesting System for Clear cutting in Larix kaempferi Stand

Eung-Jin Jeong1*, Hyun-Min Cho1, Young-Seok Lee1, Sang-Kyun Han1

(1Division of Forest Science, College of Forest & Environmental Sciences, Kangwon National University)

요약: 임목수확작업에 있어서 친환경적이고 안전한 작업을 위해서는 벌채지의 임황 및 지황을 고려한 적정한 목재수확시스템의 선정이 필수적이라 할 수 있다. 하지만 국내에서는 획일적으로 굴삭기 우드그랩을 이용한 단목수확시스템이 적용되고 있으며, 이러한 시스템은 토양환경피해, 원목 가치 및 품질 저하, 벌채부산물 수집 비용 증가 등 여러 가지 문제점이 야기하고 있다. 따라서 본 연구에서는 경사지의 낙엽송 임분을 대상으로 동일 임분에서 굴삭기 우드그랩을 이용한 단목수확시스템과 타워야더 Koller K301-4를 이용한 전목수확시스템 간의 임목수확작업 생산성 및 비용을 비교·분석하였다. 벌도작업 생산성은 전목수확시스템이 단목수확시스템보다 약 21% 높게 나타났으나, 조재작업과 집재작업의 생산성은 단목수확시스템에서 각각 약 33%와 78% 더 높게 나타났다. 총 작업생산성은 단목수확시스템이 9.1㎥/hr로 전목수확시스템의 6.1㎥/hr보다 약 67% 높게 나타났으며, 총 작업비용은 단목수확시스템이 22,439원/㎥으로 전목수확시스템의 44,256원/㎥ 보다 약 51% 저렴한 것으로 분석되었다. 하지만 향후 가선집재시스템의 작업생산성 향상과 함께 환경피해에 따른 사회적 비용 및 효율적인 벌채부산물 수집을 고려한다면, 경사지에서 효율적인 목재수확을 위해서는 전목수확 작업시스템의 적극적인 적용이 고려되어야 할 것이다.

Abstract: There is necessary to select a proper forest machine and harvesting system considering the harvesting stand and site conditions for the safe operations and environmental impacts. In South Korea, cut-to-length harvesting system using wood-grab has been uniformly applied, but this system also cause various problems such as impacts of soil environment, value loss of log, and increase of harvesting costs for woody residue. In this study, the operational productivity and cost between the cut-to-length and whole-tree harvesting system were comparatively evaluated in Larix kaempferi Stand. As a result, the operational productivity of felling operation in whole-tree harvesting system showed 33% higher than in cut-to-length harvesting system. The operational productivity of bucking and yarding operation in cut-to-length harvesting system showed each of 33% and 78% higher than in whole-tree harvesting system, respectively. The overall operational productivity of the cut-to-length harvesting system was calculated as 9.1㎥/hr, which was 67% higher than 6.1㎥/hr of the whole-tree harvesting system. The overall harvesting cost of the cut-to-length harvesting system was calculated as 22,439won/㎥, which was 51% more competitive than 44,256won/㎥ of the whole-tree harvesting system.