땅밀림 관리대상지 모니터링에 관한 연구

양대성1*, 김봉기1, 김준희1, 이상훈1, 이진호2, 장태호2

(1한국치산기술협회, 2산림청)

A Study on the Montoring of land land creep areas

Daeseong Yang1*, Bongki Kim1, Junhee Kim1, Sanghoon Lee1, Jinho Lee2, Taeho Jang3

(1Korea Association of Forest Enviro-conservation Technology, 2Korea Forest Service)

요약 : 산림청은 땅밀림 발생지역의 선제적 대응차원에서 2018년 땅밀림 기초조사를 통하여 전국 약 18만여개소를 추출 후 우선순위에 따라 2019년부터 매년 약 2천개소씩 땅밀림 실태조사를 실시 중이다. 처음 땅밀림 실태조사를 실시했던 2019년에는 땅밀림 관리대상지가 총 38개소로 도출되었다. 이 중, 집중관리대상지는 19개소로 나타났는데 2023년 6월 당시, 4개소는 무인원격감시시스템을 설치하여 관리 중이었다. 땅밀림 현상은 재발성이 강하기 때문에 지속적으로 변위량을 관측하는 것이 대단히 중요하다. 따라서 15개 대상지의 변위량을 파악하기 위해 말뚝박기 방법으로 집중호우 발생 전, 후로 구분하여 연 2회 모니터링을 실시하였다. 측정방법은 정삼각형의 조사구를 땅밀림 현상인 균열, 단차, 수목이상생장 등의 발생지점 중심에 설치하여 변위를 파악하였다. 정삼각형의 조사구 각 꼭지점 부분에 말뚝을 설치하였고, 꼭짓점 간격은 7m, 위 꼭짓점과 아래 선분은 6m 간격으로 설치하였다. 변위 발생량은 줄자를 활용하여 최초 설치 시의 말뚝간격과 설치 이후의 말뚝간격을 비교하는 방법을 활용하였고, 동시에 각 꼭짓점에서 GPS 좌표를 획득 후 Arc gis를 통해 변위량을 관찰하였다. 그 결과, 줄자를 활용하여 변위량을 파악한 방법은 설치된 말뚝이 처음 설치한 위치에 있는 것으로 조사되어 변위 발생은 없었던 것으로 나타났다. 그러나 GPS 좌표를 중첩시켜 파악한 방법은 15개소 중 15개소 모두 일치하지 않았다. 이는 GPS좌표 취득 시 수관 영향 때문에 오차범위가 ±20m 이상 발생하여 말뚝의 위치가 불일치한 것으로 판단된다.

Abstract : The KFS, as a proactive measure to address land creep areas, conducted a basic survey of land creep in 2018, identifying approximately about 180,000 locations nationwide. Based on priority, they have been conducting a detailed land creep survey of about 2,000 locations each year since 2019. In 2019, the first year of the detailed land creep survey, a total of 38 land creep management sites were identified. Among these, 19 sites were designated as high-priority management areas. As of June 2023, four of these sites were being managed using an land creep monitoring system. Because land creep have a high likelihood of recurrence, it is extremely important to continuously monitor the amount of displacement. Therefore, to understand the displacement of the 15 targeted sites, monitoring was conducted twice a year, before and after heavy rainfall events, using the pile by monitoring method. The measurement method involved setting up an equilateral triangle survey plot centered on points where land creep areas such as cracks, scarp, and abnormal tree growth were observed, to determine displacement. Pile were installed at each vertex of the equilateral triangle survey plot, with the distance between the vertices set at 7m. The upper vertex and the lower segment were spaced 6m apart. The displacement amount was determined by comparing the distance between the stakes at the time of initial installation with the distance after installation using a measuring tape. Additionally, GPS coordinates were obtained at each vertex, and displacement was monitored through Arc gis. As a result, the method of determining displacement using a measuring tape showed that the in stalled pile remained in their original positions, indicating no displacement occurred. However, the method identified by overlapping GPS coordinates did not match all 15 of the 15 locations. The reason for this is that the location of the stake is inconsistent due to the occurrence of an error range of ±20m or more due to the influence of the crown when acquiring GPS coordinates.

Key words : Land creep, Pile by monitoring, Land creep management, Triangle survey plot

사사 : 본 연구는 산림청의「2023년 전국 땅밀림 우려지 현장조사 및 물리탐사기법 고도화 연구」용역에 의하여 이루어진 것입니다.