완·중경사지에서 목재생산 방식에 따른

목재수확 작업 생산성 및 비용 비교·분석

김태형1*, 오재헌2, 조현민1, 한상균3

(1강원대학교 산림경영학과, 2국립산림과학원 산림기술경영연구소, 3강원대학교 산림과학부)

Comparative Analysis of Productivity and Costs of Timber Harvesting Methods on Moderately Steep Terrain

Taehyung Kim1*, Jae-Heun Oh2, Hyun-Min Cho1, Sang-Kyun Han3

(1Department of Forest Management, Kangwon National University,

2Forest Technology and Management Research Center, National Institute of Forest Science,

3Division of Forest Science, Kangwon National University)

요약: 국내 대부분의 목재수확 작업은 체인톱과 우드그랩을 활용한 단목생산 방식으로 이루어지고 있다. 이러한 작업 방식은 작업 생산성이 높은 반면, 장재 생산 및 부산물 수집이 어려우며 특히 벌도 작업 시 작업안전에 취약한 것으로 보고되고 있다. 이러한 문제점을 보완하기 위해 최근에는 전목생산 시스템의 도입이 요구되고 있다. 따라서, 본 연구에서는 완·중경사지인 1.5ha 낙엽송림에서 단목생산 시스템(벌도: 체인톱, 집재: 우드그랩, 조재: 체인톱)과 전목생산 시스템(벌도: 그래플쏘, 집재: 클램벙크 스키더, 조재: 프로세서)의 생산성과 비용을 비교·분석하였다. 그 결과, 단목생산 시스템의 벌도·집재·조재작업의 생산성은 각각 28.9m3/PMH, 5.8m3/PMH, 11.6m3/PMH으로, 작업비용은 각각 1,738원/m3, 14,768원/m3, 4,331원/m3으로 산출되었다. 전목생산 시스템의 벌도·집재·조재작업의 생산성은 각각 12.4m3/PMH, 8.9m3/PMH, 13.5m3/PMH으로, 작업비용은 각각 7,209원/m3, 13,787원/m3, 6,375원/m3으로 분석되었다. 두 시스템의 작업비용을 비교해보면, 단목생산 시스템(20,838원/m3)이 전목생산 시스템(27,371원/m3)보다 약 24% 저렴하였다. 본 연구 결과는 단목 및 전목생산 시스템의 작업 생산성과 비용만 분석한 것으로, 향후 장재 생산을 통한 원목 가치 증대를 고려한 추가 연구가 필요할 것으로 사료된다.

Abstract: Most timber harvesting operations in Korea are conducted using a cut-to-length (CTL) system involving chainsaws and wood grabs. While this method is cost-effective for timber harvesting, it is challenging for producing long logs and collecting logging residue with the low safety by chainsaw felling. To address these issues, the introduction of whole-tree (WT) harvesting systems is emerging as a solution. Therefore, this study compares the productivity and costs of the CTL system (felling: chainsaw, yarding: wood grab, processing: chainsaw) and the WT system (felling: grapple saw, skidding: clambunk skidder, processing: processor) in a 1.5ha Japanese larch stand on moderately steep terrain. The results showed that the productivity of felling, yarding, and processing for the CTL system was 28.9m³/PMH, 5.8m³/PMH, and 11.6m³/PMH, respectively, with costs of 1,738 KRW/m³, 14,768 KRW/m³, and 4,331 KRW/m³, respectively. For the WT system, the productivity of felling, skidding, and processing was 12.4m³/PMH, 8.9m³/PMH, and 13.5m³/PMH, respectively, with costs of 7,209 KRW/m³, 13,787 KRW/m³, and 6,375 KRW/m³, respectively. Comparing the costs of the two systems, the CTL system (20,838 KRW/m³) was 24% cheaper than the WT system (27,371 KRW/m³). This study focuses solely on the productivity and costs of the CTL and WT systems, indicating the need for further research that considers the enhancements in utilization and value of timber through the long log production.

Keywords: cut-to-length, whole-tree, clambuck skidder, grapple saw

사사: 본 연구는 산림청 산림과학기술 출연 연구개발사업(No. 2023491B10-2425-AA02)의 지원에 의해 이루어진 것임.