생태복원을 위한 산지계류 지형 변화 분석

김원호1*, 이학준1, 서준표2, 임성호1, 김지윤1

(1상지대학교 조경산림학과, 2국립산림과학원 산사태연구과)

Assessing Topographic Changes in Mountain Streams

for Ecological Restoration

Wonho Kim1*, Hakjun Rhee1, Junpyo Seo2, Seong Ho Lim1, Jeeyoon Kim1

(1Department of Forest Landscape Architecture, Sangji University,

2Landslide Division, National Institute of Forest Science)

요약: 최근 기후위기로 인해 다양한 산림 교란 및 훼손이 일어나고 있으며, 산림생태계 복원의 중요성이 대두되고 있다. 하지만 우리나라에서 산지계류 생태복원에 대한 연구는 찾아보기 힘들다. 본 연구는 계류 횡단면 및 종단면 지형 변화를 측정하여 산림 교란(산불, 벌목, 휴양) 및 지질(화성암, 변성암, 퇴적암) 등에 따른 산지계류 물리적 환경변화를 이해하려고 하였다. 이를 위해 국립산림과학원에서 모니터링 중인 6개의 유역(거창군, 김천시 대리, 경산시, 성주군, 김천시 유성리, 포항시)에 대해 사방댐 상하부, 직선, 곡선 구간, pool, 특이 지점 등 총 103개 지점(유역별 15∼21개)의 횡단면 및 종단면을 2022∼2024년 매년 Global Navigation Satellite System (GNSS) 측량기를 사용하여 측량하였다. 측량지점 횡단면은 계류 직각방향 25cm 간격으로 특이점(경사 급변 지점)은 추가로 측량하였으며, 종단면은 상하류 최저점을 측량하여 횡단면 최저점과 비교하여 산출하였다. 그 결과 횡단면 및 종단면의 변화를 수치화하여 비교할 수 있었다. 하지만 각 지점에 대한 토석류의 이동 및 변화를 이해하기 위해 계상의 토석류 입도분포에 대한 조사가 필요하다고 판단된다. 본 연구결과를 추후 각 측량지점 계상 및 계안 식생조사 자료와 함께 비교·분석한다면 산지계류 변화를 이해하고 생태복원을 위한 기초자료로 활용할 수 있을 것이다.

Abstract: Recent years there are various forest disturbances and degradation due to climate crisis. and thus importance of forest ecosystem restoration rises. This study measured stream cross- sectional and profile changes and contributed to understanding changes in physical environment of mountain streams with respect to forest disturbances (forest fire, logging and recreation) and geology (granite, metamorphic and sedimentary rocks). The six watershed sites (Geochang-gun, Gimcheon-si Dae-ri, Gyeongsan-si, Seongju-gun, Gimcheon-si Yuseong-ri and Pohang-si) monitored by National Institute of Forest Science were selected to survey cross-sections and profiles yearly from 2022 to 2024 using GNSS survey equipment from a total of 103 locations (15∼21 locations/ watershed) which are up and downstream of erosion control dams, straight and meandered sections, pools, and special points. For cross-sections every 25cm and special points (abrupt slope changes) were measured perpendicular to stream flow. The profiles were calculated by measuring up and downstream low points and comparing them with the lowest point from the cross-sections. As a result, changes in cross-sections and profiles were quantified and compared. However, particle size distribution of streambed is needed to further understand moves and changes in stream sediment at each point. This study warrants investigation on streambed and side vegetation at each location, which can be used for understanding changes in mountain streams and used as a background information for ecological restoration.

사사: 본 연구는 2024년도 국립산림과학원의 지원을 받아 이루어진 것임(2024040D352-00).