산불예방 숲 가꾸기를 통한 산림 내 연료량 변화

장미나1*, 권춘근1, 한송희1, 김성용2

(1국립산림과학원 산불연구과, 2국립안동대학교 산림과학과)

Change of Fuel Load in Pinus densiflora Stand on the Thinning for Forest Fire Prevention

Mina Jang1*, Chun Geun Kwon1, Song Hee Han1, Sung Yong Kim2

(1Division of Forest Fire, National Institute of Forest Science,

2Department of Forest Science, Andong National University)

요약: 본 연구는 대형산불이 많이 발생하는 강원도 영동지역의 소나무림을 대상으로 임분밀도 조절에 따라 산림 내 연료량이 어떻게 변화하는지를 파악하고자 하였다. 시간 경과에 따른 변화를 파악하기 위해 강원도 고성군에 위치한 소나무림을 대상으로 모니터링구를 설치하였으며, 임분밀도 조절을 위해 본 수 대비 20%, 40%의 솎아베기를 실시한 처리구와 솎아베기를 하지 않은 대조구를 설치하였다. 설치 후 3년간 모니터링한 결과 낙엽, 낙지, 관목 등 지표층 연료량은 20% 처리구 2.11kg/m2, 40% 처리구 2.02kg/m2, 대조구 2.31kg/m2으로 40% 처리구가 가장 적었다. 대형산불이 확산하는 과정에서 탈 물질이 되는 수관층 연료량은 20% 처리구 1.42kg/m2, 40% 처리구 0.96kg/m2로 대조구 1.75kg/m2과 비교하여 감소하였다. 특히 수관화 확산 시 잎과 1cm 이하의 가지는 전소되므로 연소가능한 연료라고 정의하고 있으며, 수관층 연소가능 연료량은 20% 처리구 1.19kg/m2, 40% 처리구 0.77kg/m2로 대조구 1.68kg/m2과 비교하여 40% 처리구가 2배 정도 감소하였다. 산불예방 숲 가꾸기 시 산림 내 층위별 연료량이 감소함에 따라 산불확산 저감에 영향을 미칠 것으로 판단되며, 향후 지속적인 모니터링을 통해 산림 내 연료량뿐만 아니라 임목, 식생 등의 변화 전반을 조사하여 산불예방 숲 가꾸기의 긍정적 효과를 검증하고자 한다.

Abstract: This study analyzes the changes in forest fuel load resulting from stand density control in pine forests in the Yeongdong region of Gangwon Province. To monitor temporal changes, monitoring plots were established in Gosung County, Gangwon Province. To manipulate stand density, we conducted thinning treatments at 20% and 40% relative to basal tree density, along with establishing control plots without thinning. Over a 3-year monitoring period, surface fuel loads including litter, duff, and shrubs were observed 20% treatment had 2.11kg/m², 40% treatment had 2.02kg/m², and control had 2.31kg/m², with the 40% treatment showing the lowest load. During the spread of large forest fires, the amount of crown fuel transforming into embers decreased, with the 20% treatment at 1.42kg/m² and the 40% treatment at 0.96kg/m², compared to 1.75kg/m² for the control. Especially, leaves and branches ≤1cm in diameter are considered combustible fuel during crown fire spread. The amount of combustible crown fuel was 1.19kg/m² in the 20% treatment and 0.77kg/m² in the 40% treatment, showing approximately a twofold decrease compared to 1.68kg/m² in the control. Reduced fuel loads across forest layers are expected to mitigate forest fire spread during fire prevention forest management. Through future continuous monitoring, we aim to investigate changes not only in fuel loads within forests but also in individual tree, vegetation, and other aspects, validating the positive effects of forest management for wildfire prevention.

Keyword: forest fire, forest fuel, fuel treatment