광 및 토양수분이 개가시나무(Quercus gilva)와 종가시나무(Q. glauca)의 생리적 반응에 미치는 영향

이승준1*, 박재훈1 유영한1

(1국립공주대학교 생명과학과)

Effects of Shading and Drought Treatment on the Physiological Responses of Quercus gilva and Q. glauca

Seung-Jun Lee1*, Jae-Hoon Park1, Young-Han You1

(1Department of Biological Sciences, Kongju National University)

요약: 제주도 곶자왈 지역에 자생하는 개가시나무와 종가시나무의 광과 수분에 대한 생리적 특성을 파악하고자 시도하였다. 이를 위해 광 조건을 세 단계로 조절하고, 27일간 단수(건조) 처리하여 광합성률, 증산률과 수분이용효율을 측정하고 분석하였다. 그 결과, 두 종은 광량 감소에 따라 광합성률과 증산률이 뚜렷하게 감소하였으며, 특히 음지 환경(광 2%)에서는 암호흡이 나타났다. 이는 두 종이 호광성 식물임을 나타낸다. 수분이용효율은 두 종에서 서로 다른 변화를 보였다. 개가시나무는 광량이 감소할수록 수분이용효율이 뚜렷하게 감소한 반면, 종가시나무는 전광과 중간 광량(28%)에서 유사한 수분이용효율을 유지하였다. 이는 전광에서 종가시나무의 증산률이 높았기 때문이다. 또한, 건조 강도가 증가함에 따라 토양수양함량이 감소하였으며, 토양수분함량이 약 13%에 도달한 13일까지 두 종은 광합성률의 일시적 회복반응을 보였으나, 이후 낮은 수준을 유지하였다. 이를 통해 두 종은 건조 환경에서도 일정 수준의 생리적 회복력을 가짐을 알 수 있었다.

Abstract: A study was conducted to investigate the physiological characteristics of Quercus acuta and Quercus salicina, which are native to the Gotjawal region of Jeju Island, in response to light and water conditions. To achieve this, light was adjusted to three different levels, and a 27-day drought treatment was applied. Subsequently, photosynthesis rate, transpiration rate, and water use efficiency were measured. As a result, both species showed a significant decrease in photosynthesis rate and transpiration rate with reduced light intensity. In particular, dark respiration was observed in shaded conditions (2% light), indicating that these species are heliophilic plants. Additionally, as drought intensity increased, soil moisture content decreased, and on the 13th day, when soil moisture reached approximately 13%, the physiological recovery period of both species was identified. This suggests that both species possess a certain level of physiological resilience in dry environments.

사사: This work was supported by Korea Environmental Industry & Technology Institute (KEITI) through Wetland Ecosystem Value Evaluation and Carbon Absorption Value Promotion Technology Development Project, funded by Korea Ministry of Environment (MOE) (2022003630003).