임도 시설에 따른 현행 단목수확시스템의 생산성 및 비용 분석

최윤성*, 황진성, 문호성

(국립산림과학원 산림기술경영연구소)

Productivity and Cost of Conventional Cut-to-Length Harvesting System by Effect of Forest Road Facilities

Yun-Sung Choi*, Jin-Seong Hwang, Ho-Seong Mun

(Forest Technology and Management Research Center, National Institute of Forest Science)

요약: 본 연구는 임도의 시설 효과를 파악하기 위해 임도 시설 유·무에 따른 현행 단목수확시스템을 적용한 생산성 및 비용을 비교 분석하였다. 연구대상지는 춘천국유림관리소(강원 화천군 하남면 계성리 산1-2) 관할에 위치한 모두베기 작업지로 주요 수종은 낙엽송(Ⅴ영급)이고, 임목축적은 205.6m³/ha, 평균 경사는 29.6°이다. 단목수확작업방법으로 임도 시설이 있을 시 벌도 및 조재작업과 집재작업으로 이루어졌으며, 이는 임도가 없을 시 보다 작업 현장에 접근이 용이하고, 작업 공정이 적어 생산성에 유리한 장점이 있다. 또한 임도 시설이 없을 시에는 작업로 개설 작업, 벌도 및 조재작업, 집재작업, 소운반작업으로 이루어졌다. 분석 결과, 임도 시설이 있을 시 생산성 및 비용은 벌도 및 조재작업이 2.9 ㎥/시간, 16,554원/㎥, 집재작업이 11.5 m³/시간, 7,245원/㎥으로 총 비용은 23,799원/㎥로 나타났다. 임도 시설이 없을 시 작업로 개설 작업이 19.6 m/시간, 8,608원/m³(4,069원/m, ㎥으로 환산), 벌도 및 조재작업과 집재작업의 생산성 및 비용은 임도 시설이 있을 시와 동일하게 적용하였고, 소운반작업은 10.7 m³/시간, 14,881원/m³(거리 700m)로 총 비용은 47,288원/m³로 나타났으며, 임도 시설 효과에 따른 작업 비용의 차이는 약 23,489원/m³로 분석되었다.

Abstract: The study sites were clear-cutting operations managed by the Chuncheon National Forest Station, located at Mountain 1-2, Gyeseong-ri, Hanam-myeon, Hwacheon-gun, Gangwon Province. The major tree species was Larix kaempferi in the age class Ⅴ, with a site volume of 205.6 m³/ha and an average slope of 29.6°. In the with of forest road facilities, the operations included felling and processing and yarding. The with of forest road facilitated site access, reduced operational steps, and improved productivity. Also, In the without of forest road facilities, the operations included skid trail construction, felling and processing, yarding and forwarding. The analysis showed that with forest roads, the productivity and cost were 2.9 m³/hr and 16,554 KRW/m³ for felling and processing operations, and 11.5 m³/hour and 7,245 KRW/m³ for yarding, with a total cost of 23,799 KRW/m³. Without forest roads, skid trail construction productivity were 19.6 m/hr and 8,608 KRW/m³ (4,069 KRW/m when converted to m³). The productivity and cost of felling, processing, and yarding operations were the same as when forest roads were available. For forwarding (distance of 700 m), the productivity and cost were 10.7 m³/hr and 14,881 KRW/m³, with a total cost of 47,288 KRW/m³. Therefore, the cost difference attributable to forest road effect was approximately 23,489 KRW/m³.

Keywords: forest roads, cut-to-length, harvesting system, productivity and cost

사사: 본 연구는 국립산림과학원 연구과제(FO0300-2023-01-2023)에 의해 수행되었음.