토양 컬럼실험을 통한 불포화 투수계수 추정

이시은1*, 봉태호1, 정은수1, 변지섭1

(1충북대학교 산림학과)

Estimation of Unsaturated Hydraulic Conductivity by Soil Column test

Sieun Lee1*, Taeho Bong1, Eunsoo Jeong1, Jiseop Byeon

(1Department of Forest Science, Chungbuk National University)

요약: 불포화 투수계수는 불포화토의 가장 중요한 특성 중 하나로 불포화토 내 물의 흐름을 파악하기 위해서는 이를 정확하게 예측할 필요가 있다. 일반적으로 불포화 투수계수는 지반이 함유하고 있는 함수비에 영향을 받으며, 함수비가 증가할수록 물의 이동이 원활해져 투수계수 또한 증가하는 경향을 보인다. 따라서 함수비에 따른 불포화토의 투수계수를 추정하기 위해서는 많은 시간과 노력이 요구되며, 일반적으로 함수특성곡선의 모델 변수를 활용한 간접적인 추정 방법이 사용되고 있다. 하지만 선행연구에 따르면 여러 가지 영향 인자들로 인해 실제 불포화 투수계수와 모델을 통한 예측값 사이에 오차가 발생하는 것으로 나타났다. 따라서 본 연구에서는 세 가지 토양에 대한 함수특성곡선을 기반으로 불포화 투수계수를 추정하고, 이를 증발법 및 컬럼실험을 통하여 도출된 불포화 투수계수와 비교·분석하였다.

Abstract: The unsaturated permeability coefficient is one of the most important properties of unsaturated soil, and it is necessary to accurately predict the flow of water in the unsaturated soil. In general, the unsaturated permeability coefficient is affected by the moisture content of the ground, and as the water content increases, the water movement becomes smooth and the permeability coefficient tends to increase. Therefore, estimating the permeability coefficient of the unsaturated soil according to the water content ratio requires a lot of time and effort, and in general, an indirect estimation method using model variables of the water characteristic curve is used. However, prior research has shown that errors occur between the actual unsaturated permeability coefficient and the predicted values through the model due to various influencing factors. Therefore, in this study, the unsaturated permeability coefficient was estimated based on the water characteristic curve for the three soils, and this was compared and analyzed with the unsaturated permeability coefficient derived through evaporation and column experiments.

사사: 본 성과물은(논문, 산업재산권, 품종보호권 등)은 농촌진흥청 신농업기후변화대응체계구축사업 (세부과제번호 : RS-2023-00219113)의 지원을 받아 수행되었음.