경북북부 자연사면 산사태 환경인자 특성분석 및 대책 마련

유광진*, 김동엽

(대구대학교 산림자원학과)

Analysis of Environmental Factors and Preparation of Countermeasures for Shallow Landslides on Natural Slopes in Northern Gyeongsangbuk-do in South Korea

Gwangjin Yu*, Dohun Keum Kim

(Department of Forest Resources, DeaguUnivercity)

요약: 본 연구는 산사태에 취약한 경상북도 북부 지역의 자연사면에서 산사태 발생 특성을 통계적으로 분석하고, 지역별 차이를 규명하며 관리 방안을 제시하고자 하였다. 연구 대상지는 2019년부터 2023년까지 발생한 산사태 지역을 위성·항공사진 분석 후 5m×5m 그리드로 구획하였다. 발생지 셀은 총 521개(예천 96개, 봉화 309개, 문경 116개)이며, 미발생지는 행정단위(리) 산지에서 셀 1,472개를 추출하였고, 산사태 발생 인자는 고도, 사면곡률, 경사도, 모암, 토성, 영급, 경급, 임상, 방위를 활용하여 분석하였다. 이후, 통계적 유의성과 지역별 분포성을 기준으로 주요 인자를 선정하였고, 사면길이를 추가하여 지역별 특성을 비교하였다. 분석 결과, 경상북도 북부 산사태는 주로 사면곡률(–2.15), 경사도(29.04°), 임상(활엽수림), 모암(화강암류)에서 발생하는 것으로 나타났다. 지역별로 문경은 곡률(-3.28), 사면길이(69.6m), 임상(활엽수림), 모암(석회암류)에서, 예천은 곡률(-0.3), 사면길이(40.3m), 임상(활엽수림), 모암(편마암류)에서, 봉화는 곡률(-2.3), 사면길이(70.7m), 임상(침엽수림), 모암(화강암류)에서 산사태가 발생하는 경향을 보였다. 따라서, 문경은 산사태지 주변 사방댐 및 예⦁경보시스템 개선, 예천은 개선된 조기 피난 시스템 구축, 봉화는 사방댐과 같은 구조물 대책등 지역별로 차별화된 산사태 대응 대책이 필요하다.

Abstract: This study statistically analyzes the characteristics of shallow landslide occurrences on natural slopes in northern Gyeongsangbuk-do, identifies regional differences, and suggests management strategies. The study area was divided into 5m × 5m grids using satellite and aerial images of shallow landslides from 2019 to 2023. A total of 521 occurrence cells (Yecheon: 96, Bonghwa: 309, Mungyeong: 116) and 1,472 non-occurrence cells were extracted from mountainous areas at the administrative village (ri) level. Landslide factors analyzed include elevation, slope curvature, slope gradient, bedrock, soil texture, forest age, diameter, type, and aspect. Significant factors were selected based on statistical relevance and regional distribution, with slope length added to compare regional characteristics. Shallow landslides primarily occurred in areas with slope curvature (-2.15), gradient (29.04°), broadleaf forests, and granite bedrock. Regionally, landslides occurred in Mungyeong in areas with high curvature (-3.28), slope length (69.6 m), broadleaf forests, and limestone; in Yecheon in areas with low curvature (-0.3), slope length (40.3 m), broadleaf forests, and gneiss; and in Bonghwa in areas with curvature (-2.3), slope length (70.7 m), coniferous forests, and granite. Therefore, region-specific measures are needed: Mungyeong requires debris dam and early warning systems; Yecheon needs an enhanced early evacuation system; and Bonghwa requires structural measures like debris dams.