산화촉매분획 반응 투입 촉매 차이에 따른 리기테다소나무의

액상화 효율 분석

장수경1*, 박미진1

(1국립산림과학원 임산소재연구과)

Investigation of Biomass Dissolution Efficiency According to Catalyst Types in Oxidative Catalytic Fractionation of Pinus rigida × P. taeda

Soo-Kyeong Jang1*, Mi-Jin Park1

(1Division of Forest Industrial Materials, National Institute of Forest Science)

요약: 리그닌은 석유 기반 화학 물질을 대체할 수 있는 친환경 원료로 인식되고 있으나, 회수한 리그닌의 구조적 불균일성으로 인해 활용도가 떨어지는 문제점을 가지고 있다. 이를 극복하기 위해 다양한 방법의 리그닌 해중합 기술이 개발되었으며, 최근 산화촉매분획은 리그닌 단량체를 비교적 높은 선택성으로 확보할 수 있어 큰 주목을 받고 있다. 본 연구에서는 국내 자생 침엽수종인 리기테다소나무(Pinus rigida × P. taeda)를 활용하여 산화촉매분획을 실시하고 리그닌 단량체 추출과 밀접한 연관이 있는 액상화 효율을 분석하였다. 또한 산화촉매분획에 일반적으로 투입되는 염기촉매와 산화제가 단일 투입 조건을 설계하여 촉매 투입 여부가 액상화 효율 변화에 미치는 영향을 분석하였다.

Abstract: Lignin is recognized as an eco-friendly raw material capable of replacing petroleum-based chemicals; however, its practical utilization remains limited due to the structural heterogeneity of the recovered lignin. To overcome this challenge, various lignin depolymerization technologies have been developed. Recently, oxidative catalytic fractionation has garnered significant attention for its ability to secure lignin monomers with relatively high selectivity. In this study, oxidative catalytic fractionation was performed using Pinus rigida × P. taeda, a coniferous species native to Korea, to analyze biomass dissolution efficiency, which is closely linked to the extraction of lignin monomers. Furthermore, experimental conditions were designed to involve the single addition of base catalysts and oxidants—components typically employed in oxidative catalytic fractionation—to evaluate how the presence or absence of each catalyst type influences changes in the biomass dissolution efficiency.

사사: 본 연구는 국립산림과학원 일반연구사업(FP0701-2025-01-2026)의 지원을 받아 이루어졌습니다.