산지지형 특성을 반영한 산림유역 구축 및 활용 방안

-충청북도 충주시를 대상으로-

김종민1*, 금도훈1, 민수희1, 손학기2, 송정은1

(1한국산지보전협회 산지정책연구센터, 2한국농촌경제연구원 산림경제연구실)

Development and Application of Forest Watersheds Based on Mountainous Terrain Characteristics
- A Case Study of Chungju-si, Korea -

Jongmin Kim1*, Dohun Keum1, Suhui Min1, Hakgi Sohn2, Jungeun Song1

(1Forestland Policy Research Center, Korea Forest Conservation Association,

2Office of Forest Economic Research, Korea Rural Economic Institute)

요약: 산림의 효율적인 관리·보전과 합리적인 이용을 위해서는 행정 경계나 임상 중심이 아닌, 지형과 집수 구조를 반영한 유역 단위의 공간관리체계 구축이 필요하다. 특히 우리나라와 같이 산림비율이 높은 지역에서는 복잡한 산지지형 특성을 반영한 유역 중심의 공간단위 설정이 필요하다. 그러나 국내에서 주로 활용되는 유역은 하천망 중심으로 생성되어 수자원을 관리하는 목적으로 제작되는 경우가 많아, 유역 규모가 상대적으로 커 소규모 지형을 충분히 반영하지 못하는 한계가 존재한다. 이러한 국가·지방하천 등 주요 하천 중심의 유역은 하천망과 유출지점을 기준으로 공간 단위가 설정되어 산림의 세밀한 지형 구조를 반영하기 어려우므로, 본 연구에서는 산림의 지형 특성을 반영하는 ‘산줄기내포유역’의 유역 분류 방법을 제안하고, 그 적용 결과와 활용 방안을 제시하고자 한다. 충북 충주시(총 면적 98,350 ha)를 대상으로 산줄기내포유역을 구축한 결과, 1차 지류유역은 총 1,889개로, 총 면적 77,994 ha, 평균 면적 41.3 ha(4.4~1,490.7 ha)로 도출되었으며, 2차 지류유역은 총 2,935개로, 총 면적 44,244 ha, 평균 면적 15.1 ha(3.6~303.6 ha)로 분석되었다. 산줄기내포유역은 산지의 지형 구조와 능선을 기반으로 형성되는 유역 단위로서, 소규모 산림지역의 집수 구조와 유역 경계를 보다 사실적으로 표현할 수 있다는 점에서 기존 유역 구분 방식과 차별성을 가진다. 또한, DEM 기반 래스터 자료의 특성상 유역 경계가 격자 단위로 생성되는 문제가 발생하는데, 본 연구에서는 외형 편집과 임상도 기반의 분류 과정을 거쳐 보다 자연스러운 산림유역을 구축하였다. 이러한 산림유역은 산림재난 예방을 비롯하여 산림경영, 수원함양, 경관 조성 등 효율적인 관리 및 계획 수립을 위한 기초 공간자료로 활용될 수 있을 것으로 기대된다.

Abstract: Efficient forest conservation, management, and sustainable use require a watershed-based spatial management framework that reflects topographic and catchment characteristics rather than administrative boundaries or forest type–based classifications. In regions with a high proportion of forest cover, such as Korea, it is particularly important to establish watershed-based spatial units that adequately represent complex mountainous terrain. However, watersheds commonly applied in Korea are primarily delineated based on river networks for water resource management purposes, resulting in relatively large units that fail to capture fine-scale forest terrain characteristics. Watersheds centered on major national and local rivers rely on river networks and outlet points, which limits their applicability for detailed forest spatial management. To address these limitations, this study proposes a watershed classification method termed the ridge-nested watershed, which reflects forest terrain characteristics. The ridge-nested watershed was constructed for Chungju-si, Korea(total area: 98,350 ha). As a result, 1,889 first-order sub-watersheds were delineated, with an average area of 41.3 ha(4.4–1,490.7 ha), while 2,935 second-order sub-watersheds were identified, with an average area of 15.1 ha(3.6–303.6 ha). Although watershed boundaries derived from DEM-based raster data inherently exhibit grid-based characteristics, this study constructed more natural forest watershed units through boundary editing and forest type map–based classification. The resulting ridge-nested forest watersheds are expected to serve as fundamental spatial data for forest disaster prevention, forest management, water yield enhancement, and landscape planning.