임도에 따른 현행 및 고성능 임업기계 단목수확시스템의

생산성․비용 비교 분석

최윤성1*, 황진성1, 전현준1, 이은재2

(1국립산림과학원 산림기술경영연구소, 2영남대학교 산림자원학과)

Productivity and Cost between Conventional and High-Performance Mechanized Cut-to-length Harvesting Systems by Forest Road

Yun-Sung Choi1*, Jin-Seong Hwang1, Hyoen-Jun Jeon1, Eun-Jai Lee2

(1Forest Technology and Management Research Center, National Institute of Forest Science,

2Department of Forest Resources, Yeungnam University)

요약: 본 연구는 임도 유·무에 따른 현행 및 고성능 임업기계 단목수확시스템의 생산성과 작업비용을 비교·분석하였다. 현행은 춘천국유림관리소 관할(강원 화천군 하남면 계성리 14임반)의 모두베기 작업지(낙엽송, Ⅴ영급, 330.9 ㎥/ha, 평균 경사 29.6°)를, 고성능 임업기계는 평창국유림관리소 관할(강원 평창군 봉평면 덕거리 121임반)의 모두베기 작업지(낙엽송, Ⅴ영급, 307.9 ㎥/ha, 평균 경사 30.2°)를 대상으로 실시하였다. 임도가 있는 경우 작업방법은 벌도 및 조재작업과 집재작업으로 구성되며, 임도가 없는 경우 임산물 운반로 개설과 소운반 작업이 추가된다. 분석 결과, 임도가 있는 경우 현행의 생산성·비용은 벌도 및 조재작업 2.9 ㎥/시간(16,554원/㎥), 집재작업 11.5 ㎥/시간(7,245원/㎥)으로 총 23,799원/㎥이었고, 고성능 임업기계는 벌도 및 조재작업 15.9 ㎥/시간(13,641원/㎥)로 나타났다. 임도가 없는 경우 임산물 운반로 개설작업은 현행이 19.6 m/시간(4,069원/m → 8,608원/㎥), 고성능 임업기계는 15.0 m/시간(6,567원/m → 14,975원/㎥)로 나타났다. 또한 소운반 작업(거리 700 m)은 현행 10.7 ㎥/시간(14,436원/㎥), 고성능 임업기계 14.2 ㎥/시간(15,114원/㎥)로 나타났다. 총 작업비용은 임도가 있는 경우 현행 23,799원/㎥, 고성능 임업기계 13,641원/㎥, 임도가 없는 경우 현행 46,873원/㎥, 고성능 임업기계 43,730원/㎥으로 분석되었다. 따라서 임도의 개설 효과에 따른 작업비용 차이는 현행 23,044원/㎥, 고성능 임업기계 30,089원/㎥로 분석되었다.

Abstract: This study compared the productivity and cost of conventional and high-performance mechanized cut-to-length (CTL) harvesting systems with and without forest road. The conventional system was investigated at a clear-cutting site managed by the Chuncheon National Forest Station (Compartment 14, Gyesung-ri, Hanam-myeon, Hwacheon-gun, Gangwon province), Larix kaempferi (age class V) with a site volume of 330.9 ㎥/ha and a mean slope of 29.6°. The high-performance mechanized system was investigated at a clear-cutting site managed by the Pyeongchang National Forest Station (Compartment 121, Deokgeo-ri, Bongpyeong-myeon, Pyeongchang-gun, Gangwon province), Larix kaempferi (age class V) with a site volume of 307.9 ㎥/ha and a mean slope of 30.2°. without forest road, skid trail construction productivity was 19.6 m/hr for the conventional system and 15.0 m/h for the high-performance mechanized system. The cost were KRW 8,608/m³ (KRW 4,069/m) for the conventional system and KRW 14,975/m³ (KRW 6,567/m) for the high-performance system. In addition, forwarding (Distance 700 m) showed a productivity of 10.7 m³/hr (KRW 14,436/m³) for the conventional system and 14.2 m³/hr (KRW 15,114/m³) for the high-performance mechanized system. Total operation cost were KRW 23,799/m³ (conventional) and KRW 13,641/m³ (high-performance) with forest road, and KRW 46,873/m³ (conventional) and KRW 43,730/m³ (high-performance) without forest road. Accordingly, the cost difference attributable to the forest road effect was analysed at KRW 23,044/m³ for the conventional system and KRW 30,089/m³ for the high-performance mechanized system.

Keywords: forest road, cut-to-length, conventional and high-performance mechanized, harvesting system

사사: 본 연구는 국립산림과학원 연구과제(FO0300-2023-01-2026)에 의해 수행되었음.