임도 개설이 계류수질에 미치는 영향에 관한 사례연구

김범수1*, 이상인1, Musdalifah1, 황진성2, 최윤성2, 권형근3, 서정일1

(1국립공주대학교 산림과학과, 2국립산림과학원 산림기술경영연구소,
3국립한국농수산대학교 작물⋅산림학부)

A Case Study on the Impact of Forest Road Construction on

Stream Water Quality

Beom-su Kim1*, Sang In Lee1, Musdalifah1, Jin-Seong Hwang2, Yun-Sung Choi2,

Hyeong-Keun Kweon3, Jung Il Seo1

(1Department of Forest Science, Kongju National University,

2Forest Technology and Management Research Center, National Institute of forest science,

3Department of Crops and Forestry, Korea National University of Agriculture and Fisheries)

요약: 이 연구에서는 임도 개설이 산지계류의 수질에 미치는 영향을 파악하고자 전라북도 진안군 대불리 일대 산지계류를 대상으로 임도 개설 전ㆍ중ㆍ후의 수온, 수소이온농도, 용존산소량, 전기전도도, 유속 및 탁도, 이상 6개의 수질 인자를 임도 상ㆍ하류구간에서 수집하여 그 변화를 살펴보았다. 분석 결과, 6개 인자 중 임도 개설로 인해 가장 큰 변화가 관찰된 인자는 탁도로 나타났다. 임도 개설 당해 탁도는 임도 비탈면으로부터의 토사유입으로 인해 임도 하류구간(2.37±1.73NTU)에서 상류구간(0.98±0.62NTU)에 비해 높게 나타났다(p<0.05). 그러나 임도 개설 이듬해에는 개설 중에 비해 강우량과 홍수유출량이 상대적으로 많았음에도 불구하고 오히려 탁도는 낮아졌으며(하류구간 0.42±0.25NTU, 상류구간 0.44±0.25NTU), 이는 임도 개설 이후 토사의 공급이 제한되었기 때문으로 사료된다. 이 연구를 통해 임도 개설에 의한 계류수질 변화가 임도 개설 시기로 제한되는 것을 확인할 수 있었다. 그러나 그로 인한 서식지의 회복은 더 긴 시간이 소요될 것으로 추정됨에 따라 임도 개설 시 계류로의 토사유입을 저지할 수 있는 적극적인 대책이 요구된다.

Abstract: This study examined the impact of forest road construction on stream water quality by analyzing six water quality parameters—water temperature, pH, dissolved oxygen, electric conductivity, flow velocity, and turbidity—collected from upper and lower sections of the forest road for three years (before, during, and after construction), for a stream in the national forest, Daebul-ri, Jinan-gun, Jeollabuk-do, Republic of Korea. Of the six parameters analyzed, turbidity showed the most significant change due to forest road construction. In the construction year, the turbidity was higher in the lower stream section (2.37±1.73 NTU) than in the upper stream section (0.98±0.62 NTU), likely reflecting sediment inflow generated during construction activities (p<0.05). However, in the year following the construction, the turbidity levels were lower despite the relatively larger rainfall and peak runoff discharge (0.42±0.25 NTU lower stream section; 0.44±0.25 NTU upper stream section) compared to the previous year, suggesting the limited supply of sediment following the forest road completion. Our findings indicate that the changes in stream water quality associated with forest road are limited to the construction year. However, as it is estimated that the post-construction recovery of habitat may take longer, and therefore, active measures are required to prevent sediment inflow into streams during forest road construction.

사사: 이 연구는 국립산림과학원 연구과제(FO0300-2023-01-2026)에 의해 수행되었음.