목재수확 연계 천연갱신 규모화를 위한 잔존 군상 배치 모의 연구

이용규1*, 이상태1, 윤태경2

(1국립산림과학원 산림기술경영연구소, 2국민대학교 산림환경시스템학과)

Simulation Study on the Arrangement of Retention Patches for

Scaling up Natural Regeneration Linked with Timber Harvesting

Yong Kyu Lee1*, Sang Tae Lee1, Tae Kyung Yoon2

(1Forest Technology and Management Research Center, National Institute of Forest Science

2Department of Forestry, Environment, and Systems, Kookmin University)

요약: 최근 친환경 목재수확에 대한 요구도가 증가하여 잔존목의 존치 비율이 증가함에 따라 천연갱신을 통한 주요 조림 수종의 후계림 조성이 산림자원 선순환체계 기반 구축의 대안으로 제시되고 있다. 이에 따라, 본 연구는 천연갱신 규모화를 위해 종자비산모델을 활용하여 소나무, 낙엽송의 유효비산거리를 도출하고, 천연갱신 규모화를 위한 잔존 군상 배치를 모의하였다. 종자비산모델을 통해 구축된 예측 지도를 활용하여 군상으로부터 떨어진 거리에 따른 종자 수를 예측하였다. 또한, 종자수가 거리에 따라 감소하는 과정에서 변곡점을 유효 비산거리로 정의하였으며, 소나무는 20m, 낙엽송은 24m로 도출되었다. 유효비산거리를 활용하여 잔존 군상 배치를 모의 한 결과, 각 원형 군상의 수와 배치 방법, 수림대의 존재 유무에 따라, 종자가 비산되는 유효 범위를 도출할 수 있었다. 모의한 가상의 시범지에서는 동일한 사업면적 내에서 수림대를 존치하고, 좁은 폭의 군상 수를 늘리는 배치가 유리하였으며, 수림대가 외곽부의 갱신 안정성을 크게 개선함을 시사하였다. 따라서, 향후 천연갱신을 위한 목재수확 설계에서는 유효 비산거리 기반의 군상 간격 설정과 외곽 완충수림대의 체계적 배치가 주요한 고려 요소인 것으로 판단된다.

Abstract: As demands for eco-friendly timber harvesting increase, leading to higher retention rates of residual trees, establishing successor forests of major plantation species through natural regeneration is being proposed as an alternative for building a sustainable cycle of forest resources. Accordingly, this study derived the effective dispersal distances of Pinus densiflora and Larix kaempferi using a seed dispersal model and simulated the arrangement of retention aggregates to scale up natural regeneration. Using prediction maps generated by the seed dispersal model, seed counts were estimated based on the distance from the aggregates. Variations in dispersal distance relative to aggregate width were minimal. The inflection point in the decline of seed density was defined as the effective dispersal distance, which was determined to be 20 m for Red Pine and 24 m for Japanese Larch. Simulations of retention aggregate arrangements using these distances allowed for the derivation of effective seed dispersal ranges based on the number and layout of circular aggregates and the presence of residual forest strips. In a virtual pilot site simulation, an arrangement that retained forest strips and increased the number of narrower aggregates within the same project area proved advantageous. This suggests that residual forest strips significantly improve regeneration stability in peripheral areas. Therefore, setting aggregate intervals based on effective dispersal distance and the systematic arrangement of outer buffer strips are judged to be critical considerations in future designs for natural regeneration-oriented forest management.