배롱나무 3년생 품종(핑크벨벳)과 자생종 탄소저장량 비교분석

김찬범1*, 김학구1, 이희준2, 임윤경1, 이성훈1, 김현철1, 권용진1

(1한국수목원정원관리원 국립세종수목원, 2다원식물원)

Comparative Analysis of Carbon Storage Capacity between 3-Year-Old Lagerstroemia indica Native Species and 'Pink Velvet' Cultivar

Chan-Beom Kim1*, Hak-Koo Kim1 ,Hee-Jun Lee2, Yun-Kyung Lim1, Seong-Hun Lee1, Hyun-Chul Kim1, Yong-Jin Kwon1

(1Korea Arboreta and Gardens Institute, Sejong National Arboretum,

2Dawon Botanical Garden Agricultural CO. Ltd.)

요약: 배롱나무는 도시숲과 정원에 자주 활용되는 아교목성 수종으로 기후위기 시대에 탄소흡수원으로 활용하기 위해서는 정확한 탄소저장량 분석이 필요하다. 기존의 배롱나무는 남부지방에 주로 식재되어왔으나 최근 여름철 조경수로 주목받고 있으며, 중부지방에도 식재가 이루어지고 있다. 하지만 내한성이 약하여 겨울철 관리가 필수적이다. 배롱나무 품종 중 핑크벨벳은 내한성을 강화한 품종으로 국내에 많은 식재가 이루어지고 있으나 탄소저장에 대한 효과분석이 이루진 바가 없다. 따라서 탄소저장량 효과를 분석하기 위해 도시숲 조성 초기에 가장많이 쓰이는 3년생을 대상으로 61본의 탄소저장량을 비교 분석하였다. 그 결과, 자생종은 61.04±31.39 gC, 핑크벨벳은 45.06±21.55 gC였으며, 뿌리지상부 비율은 자생종 0.28±0.08, 핑크벨벳은 0.23±0.06로 나타났다. 앞으로 생장단계별 분석을 통해 상대생장식을 개발할 수 있을 것이며, 이 자료를 바탕으로 연간 탄소흡수량 추정하고 도시숲의 탄소저장량을 예측에 활용할 수 있을 것이다.

Abstract: Lagerstroemia indica is a widely used small tree in urban greening. To utilize this species effectively as a carbon sink, precise carbon storage data is required. While native species are expanding into central Korea due to their value as summer landscaping trees, their low cold hardiness remains a challenge. 'Pink Velvet', a cold-hardy cultivar, is being adopted as an alternative, but its carbon sequestration efficacy lacks empirical analysis. This study evaluated the carbon storage of 61 three-year-old saplings, a common age for urban establishment. The carbon storage was found to be 61.04 ± 31.39 g C for the native species and 45.06 ± 21.55 g C for 'Pink Velvet'. The root-to-shoot (R/S) ratios were 0.28 ± 0.08 for the native species and 0.23 ± 0.06 for 'Pink Velvet', respectively. These results serve as a basis for developing allometric equations and estimating the carbon sequestration potential of urban forests.

Key words: Urban forest, Cold Hardiness, Landscpae Tree, Small tree, Carbon Stock

사사: 본 연구는 한국수목원정원관리원『정원·도시숲 탄소흡수증진을 위한 관목 탄소흡수계수 개발』기술과제의 일환으로 수행되었음