도시숲에서 측정한 높이별 미세먼지 분포 특성 –천장산을 중심으로

김평래*, 황병묵, 서홍덕

(국립산림과학원 산림보전연구부 도시숲연구센터)

Characteristics of Aerosol Distribution by Elevation Measured in Urban Forest – focused on Cheonjangsan Mountain

Pyung-Rae Kim*, Byung-Mook Hwang, Hong-Duck Sou

(Urban Forests Research Center, Department of Forest Conservation, National Institute of Forest Science)

요약 : 미세먼지는 다른 주요 대기 오염과 함께 가장 시급한 대기 오염 문제가 되었다. 도시숲은 대기 오염물질을 저감 시킴으로써, 도시 대기 환경을 향상시키는데 중요한 역할을 한다. 숲이 미세먼지를 감소시키는 방법으로는 흡수, 흡착, 차단, 침강이 있으며, 이러한 과정을 통해 대기 오염물질을 감소시킨다. 본 연구에서는 소나무 숲 내에서 높이별로 미세먼지를 농도를 측정하여 높이에 따른 미세먼지 특성을 파악하고자 하였다. PM10, PM2.5 측정은 Airpro(SGA Embedded Co. Ltd, Korea)를 사용하여, 높이별로(0.5m-하층, 1.5m- 지층, 4m-중층, 6m-상층) 측정하였다. 측정 기간동안 PM10 농도는 상층이 36.9㎍m-3, 중층이 43.2㎍m-3, 지층이 38.1㎍m-3, 하층이 32.6㎍m-3으로 나타났고, PM2.5 농도는 28.3㎍m-3, 29.5㎍m-3, 29.2㎍m-3, 26.8㎍m-3으로 각각 나타났다. 이는 미세먼지가 상층에서 하층으로 이동할 때 잎 표면에 흡수, 흡착되면서 농도가 변하는 것으로 판단된다. 도시숲 내 미세먼지의 동태 파악을 바탕으로 미세먼지 저감을 위한 도시숲의 조성 및 관리방안 수립에 도움이 될 것으로 생각된다.

Abstract: Fine particulate matter, along with other atmospheric particulate pollution, has become the most pressing air pollution concern in the country. Urban forests play an important role in improving the urban atmospheric environment by reducing atmospheric pollution. Forest can reduce PM by absorption, adsorption, blocking and deposition. In this study, we try to understand the distribution characteristics of aerosol by measurement according to the vertical position in the Pinus Koraiensis forest. The PM10, PM2.5 concentrations were measured by a mobile PM measuring device, Airpro(SGA Embedded Co. Ltd, Korea), which was installed 0.5, 1.5, 4, 6m above the ground.  The average PM10 concentration were 36.9㎍m-3, 43.2㎍m-3, 38.1㎍m-3, 32.6㎍m-3 in 6, 4, 1.5, 0.5m, respectively. PM2.5 concentration were 28.3㎍m-3, 29.5㎍m-3, 29.2㎍m-3, 26.8㎍m-3, respectively. when fine dust moves form the upper layer to the lower layer, the concentration seems to change as it was absorbed or adsorbed to the leaf surface. Based on understanding the dynamics of fine dust in the urban forests, this study can contribute to development and management of urban forests to reduce fine dust.

Keyword: Urban Forest, PM10, PM2.5, dynamics of PM

사사: 본 연구는 국립산림과학원 ‘미세먼지 발생원 대응 도시숲 조성 모델 개발’ 과제(#FE01002019032020)에서 수행한 연구 결과임