전라남도산림연구원의 사운드스케이프 특성

신용규1*, 김민희1, 박종석2, 오득실2

(1동신대학교 산림조경학과, 2전라남도산림연구원)

Soundscape Characteristics of
the Jeollanam-do Forest Research Institute

Yong-Gyu Shin1*, Min-Hee Kim1, Jong-Seok Park2, Deuk-Sil Oh2

(1Department of Forestry and Landscape Architecture, Dongshin University,

2Jeollanam-do Forest Research Institute)

요약: 전라남도산림연구원은 부지 내 공간을 활용하여 유아숲, 숲해설, 산림치유 프로그램 운영 등 산림복지 및 휴양서비스를 제공하고 있다. 이러한 공간 기반 서비스는 오감을 통해 인지되며, 특히 시청각 정보는 공간의 인식과 판단에 많은 영향을 미친다. 본 연구는 산림복지 및 휴양서비스 공간으로서 전라남도산림연구원 내 공간 유형별 소리를 측정 및 분석하여 소리 환경 특성을 다양한 물리 지수로 소개함으로써 이용자 만족도 제고를 위한 사운드스케이프 설계 기초자료를 제시하고자 하였다. 이를 위해 방문자센터에서 식산오름길까지 주요 공간별 측정 지점을 설정하고, 측정 및 녹음 후 음향지수(Leq, StdDev, L90, NbEm, EmT, REm, G), 음질지수(Loudness, Sharpness, Fluctuation Strength, Roughness, Unbiased Annoyance, Articulation Index(NHV)), 주파수특성, 타임 히스토리 등을 비교 분석하였다. 그 결과, 공간 유형(진입, 정원, 숲)에 따라 인지성(전달), 인공음, 자연음 등의 분포 특성을 설명할 수 있는 지수로 StDev, REm(%), Loudness(sone), Roughness(asper), Unbiased Annoyance (au), Articulation Index(NVH, %)가 도출되었다. 향후 이를 활용한 이용자 주관평가 등 추가 연구를 통해 서비스 만족도를 높이기 위한 사운드스케이프 설계 방법의 도입 및 제안을 구체화할 수 있을 것으로 판단된다.

Abstract: The Jeollanam-do Forest Research Institute utilizes the site to provide forest welfare and recreational services, including forest kindergartens, forest interpretation, and forest healing programs. These services are perceived through the five senses, with visual and auditory information significantly influencing spatial perception and judgment. This study aims to present foundational data for soundscape design to enhance user satisfaction by measuring and analyzing the sounds of various spatial types within the Jeollanam-do Forest Research Institute and describing the characteristics of the sound environment through various physical indices. Key points for measurement were established from the visitor center to the Siksan Orum Trail, and simultaneous measurements and recordings were taken. Acoustic indices(Leq, StdDev, L90, NbEm, EmT, REm, G), sound quality indices(Loudness, Sharpness, Fluctuation Strength, Roughness, Unbiased Annoyance, Articulation Index(NHV)), frequency characteristics, and time history were compared and analyzed. As a result, indices including StdDev, REm(%), Loudness(sone), Roughness(asper), Unbiased Annoyance(au), and Articulation Index(NHV, %) were derived to explain the distribution characteristics of recognizability(transmission), artificial sounds, and natural sounds according to spatial types(entrance, garden, forest). Future research involving subjective user evaluations using these indices is expected to facilitate the introduction and specification of soundscape design methods to enhance service satisfaction.

사사: 본 연구는 교육부와 한국연구재단의 재원으로 지원을 받아 수행된 3단계 산학연협력 선도대학 육성사업(LINC 3.0)의 연구결과입니다.