우리나라 산사태 유발 강우 특성 및 임계기준(2020-2022)

장수진*, 유송, 이기환, 서준표, 우충식, 이창우

(국립산림과학원 산사태연구과)

Characteristics of Landslide-Triggering Rainfall and Critical Rainfall Thresholds in South Korea (2020–2022)

Sujin Jang*, Song Eu, Kihwan Lee, Junpyo Seo, Choongshick Woo, Changwoo Lee

(Landslide Division, National Institute of Forest Science)

요약: 최근 기후변화에 따른 극한호우 발생으로 대규모 산사태가 빈발하여 인명피해로 이어지고 있다. 이를 해결하기 위한 비구조물 대책으로는 조기경보시스템의 운영 및 경계피난 체계의 마련 등이 있다. 조기경보시스템에 활용되는 기본적 요소는 산사태 유발 강우의 임계값으로, 산사태 발생을 예측하는 데 필수적이다. 단, 강우 임계값을 분석하기 전에 적절한 강우-산사태 관계를 파악하기 위한 산사태 발생지의 강우 및 공간자료 구축이 선행되어야 한다. 이 연구의 목적은 2020년부터 2022년까지의 최근 우리나라 산사태 유발 강우(N=2306)의 특성을 분석하고, 강우의 임계기준을 도출하는 데 있다. 먼저, 강우사상 간 최소시간 간격을 24시간, 48시간 기준으로 강우사상을 분리한 후, 시우량, 일우량, 유효강우량 등 산사태 유발 강우 특성을 분석하였다. I-D, E-D 곡선을 제시하고 분위수회기분석을 통해 강우의 임계기준을 검토하였다.

Abstract: In recent years, extreme rainfall events, influenced by climate change, have led to frequent large-scale landslides, resulting in several casualties. Non-structural measures to address this issue include implementing early warning systems and establishing evacuation plans. The critical threshold of landslide-triggering rainfall, essential for predicting landslide occurrences, is a pivotal component of early warning systems. However, before analyzing this threshold, collecting and compiling rainfall and spatial data of the landslide site is crucial for identifying the appropriate rainfall-landslide relationship. This study aimed to analyze the characteristics of landslide-triggering rainfall events (N = 2306) in South Korea from 2020 to 2022 and calculate the critical rainfall thresholds. The rainfall events were first categorized based on a minimum inter-event time (MIT) of 24 and 48 h. The characteristics of the landslide-triggering rainfall, including hourly, daily, and effective rainfall, were then analyzed. Finally, the intensity-duration (I-D) and effective rainfall-duration (E-D) curves were constructed, and critical rainfall thresholds were identified using quantile regression analysis.

Keywords: landslide-triggering rainfall, critical rainfall threshold, minimum inter-event time (MIT), I-D curve, E-D curve.