인체의 생리⋅심리지표를 활용한 사방댐 경관 평가

김범수1*, 김용래2, 김초윤1, 이상인1, 조원신1, 권형근3, 송초롱1, 서정일1

(1국립공주대학교 산림과학과, 2한국산림기술인회 산림기술연구원, 3한국농수산대학교 작물⋅산림학부)

Evaluation of Landscape Created by Erosion Control Dam Using

Physiological and Psychological Indicators

Beom-Su Kim1*, Yong-Rae Kim2, Choyun Kim1, Sang In Lee1, Won-Shin Cho1,

Hyeongkeun Kweon3, Chorong Song1, Jung Il Seo1

(1Department of Forest Science, Kongju National University, 2Korea Forest Engineer Institute,

3Department of Crops and Forestry, Korea National University of Agriculture and Fisheries)

요약: 이 연구는 사방댐의 외관(콘크리트, 돌붙임, 목재붙임)이 인간의 생리⋅심리상태에 미치는 영향을 파악하기 위해 수행되었다. 실험은 산림공학 관련 활동 경험이 전무한 34명의 대학생을 대상으로 실내에서 사방댐 이미지를 이용하여 진행되었다. 피험자들은 생리지표 측정장치를 착용한 상태로 55인치 크기의 디스플레이에서 1.4m 떨어진 위치에 착석하여 (i) 회색 화면을 1분 동안 보며 안정을 취한 후 (ii) 세 가지 사방댐 이미지 중 무작위로 하나를 1분 동안 시청하였다. 이후 (iii) 심리지표 측정을 위한 설문지를 5분간 작성하고, (iv) 다시 5분 동안의 휴식을 통해 잔여 민감도를 제거하였다. 이상의 과정은 세 가지의 사방댐 이미지 모두를 볼 때까지 3회 반복되었다. 생리지표 분석 결과, 각각의 사방댐 이미지를 보는 것으로 인해 피험자들의 심박수는 유의하게 변하지 않았다. 다만, 세 가지 사방댐 중에서 콘크리트 사방댐과 목재붙임 사방댐에 대한 피험자들의 심박수 변화량 간에는 차이를 보였다. 심리지표 분석 결과, 피험자들은 콘크리트 사방댐과 돌붙임 사방댐을 ‘인공적’으로 인식하는 반면, 목재붙임 사방댐은 ‘자연적’으로 인식하는 것으로 나타났다. 또한, 다른 사방댐에 비해 목재붙임 사방댐을 볼 때 ‘활기’를 느껴 종합정서장애 점수가 감소하였다. 그러나 그 외의 모든 심리지표는 사방댐 종류 간에 유의미한 차이가 없었을 뿐 만 아니라 세 가지 사방댐 모두에 비교적 긍정적인 인상을 갖는 것으로 나타났다. 따라서 사방댐의 설계와 시공은 경관을 고려한 외관 소재의 선정에 앞서 산지토사재해에 대한 안정성을 확보하는 것이 우선되어야 할 것이다.

Abstract: This study examined effect of differences in the exterior (concrete-exposed, stone-attached, wood-attached) of erosion control dams (ECDs) on humans. We recruited 34 university students who had no experience in forest engineering-related activities. Participants sat 1.4 m away from a 55-inch display while wearing a device for measuring heart rate (HR) and heart rate variability. They (i) took a rest while viewing a gray screen for 1 minute; (ii) viewed a randomly displayed image of one of the three ECDs’ images for 1 minute; (iii) filled out questionnaires for 5 minutes; and (iv) took a rest to wash out residual sensitivity for 5 minutes. The process was repeated three times with three different ECD images. No significant difference was found between the participants’ HRs measured before and while viewing the three ECD images, although the HRs were reduced when viewing the wood-attached ECD compared to the concrete-exposed ECD. Participants perceived the wood-attached ECD naturally but they felt the concrete-exposed and stone-attached ECDs artificially. In addition, the vigor score was increased and total mood disturbance was decreased when viewing the wood-attached ECD image. However, there were no significant differences in other indicators, and participants’ responses to the exteriors of the ECDs were positive overall. Our findings show that people do not physiologically and psychologically perceive ECDs negatively. Therefore, for the design and construction of ECDs, securing structural stability against sedimentary disasters should be a priority before selecting exterior materials considering the landscape.

사사: 본 연구는 산림청(한국임업진흥원) 산림과학기술 연구개발사업(RS-2021-KF001660)의 지원에 의하여 이루어짐