전기저항단층촬영을 활용한 야자류 수간 단면의 전기저항 분포 특성

송영근1*, 심윤진2, 김예은2, 임병호2, 강창훈3, 이경철2

(1전북대학교 임학과, 2한국농수산대학교 작물산림학부, 3국립생태원 세계식물생태부)

Spatial Patterns of Electrical Resistivity in Palm Trunk Cross Sections Using Electrical Resistance Tomography

Yeonggeun Song1*, Yun Jin Shim2, Yeeun Kim2, Byoungho Lim2, Chang-Hoon Kang3, Kyeong Cheol Lee2

(1Department of Forestry, Jeonbuk National University,

2Department of Crops and Forestry, Korea National University of Agriculture and Fisheries,

3Department of World Plant Ecology, National Institute of Ecology)

요약: 본 연구는 야자류 Butia capitata와 Phoenix canariensis의 건전한 개체를 대상으로 전기저항단층촬영(ERT)을 적용하여 수간 단면에서 나타나는 전기저항 분포 특성을 분석하였다. 분석결과, ERT를 통해 산출된 수간 단면의 저항률은 B. capitata에서 약 69-374 Ωm, P. canariensis에서 약 144-312 Ωm 범위로 나타나 일반적인 활엽수 및 침엽수 수종에 비해 전반적으로 낮은 수준을 보였다. 이러한 특성은 야자류 수간이 가지는 해부학적 구조와 생리적 특성이 전기적 특성에 반영된 결과로 해석되었다. 반경 방향 분석 결과, B. capitata에서는 중심부에서 상대적으로 높은 저항률이 나타나고 외곽부로 갈수록 감소하는 경향이 비교적 뚜렷하게 관찰된 반면, P. canariensis에서는 영역 간 저항률 차이가 상대적으로 완만하여 수종별 전기저항 분포 양상의 차이가 확인되었다. 또한, North-South 및 East-West 방향을 기준에서도 중심부 대비와 외곽부 변동성이 일관되게 유지되어, 관찰된 전기저항 분포 특성이 특정 측정 방향이나 지점 선택에 의해 형성된 결과가 아님을 확인하였다. 본 연구 결과는 야자류 수간에서도 ERT를 활용한 반경 방향 중심의 공간적 전기저항 분포 해석이 가능함을 보여주며, 일반적인 목본 수종을 기준으로 한 절대 저항률 해석의 한계와 함께 야자류 특성을 고려한 해석 기준 마련의 필요성을 시사한다. 이에 본 연구에서 제시된 결과는 향후 야자류 수간의 내부 특성 평가 및 비파괴적 진단 연구를 위한 기초 자료로 활용될 수 있을 것이다.

Abstract: The application of electrical resistivity tomography (ERT) to palm stems remains limited despite its widespread use in woody tree species. This study investigated the spatial characteristics of electrical resistivity distribution in stem cross-sections of healthy Butia capitata and Phoenix canariensis. Resistivity values ranged from approximately 69-374 Ωm in B. capitata and 144-312 Ωm in P. canariensis, which are substantially lower than those reported for typical broadleaf and coniferous trees. Radial analysis showed higher resistivity in the central region of B. capitata with a decreasing trend toward the outer region, whereas P. canariensis exhibited more moderate radial variation. Consistent central-outer contrasts and increased variability in the outer region were observed along both North-South and East-West directions, indicating that these patterns reflect intrinsic stem structure rather than measurement orientation. These results demonstrate that radial based interpretation of ERT data is applicable to palm stems, while also highlighting the limitations of applying absolute resistivity thresholds derived from woody species. The findings provide baseline information for future non-destructive assessment and monitoring of palm stem internal conditions.